**Gel Batteries (12 V/200Ah)Technical Specifications and**

|  |  |  |
| --- | --- | --- |
| **Value** | **Parameter** | **No.** |
| **- Gel Type Battery, Deep Cycle**  **- Solar Energy Applications**  **- Completely Maintenance Free.**  **- Sealed construction.** | **Type & Application** | **1.** |
| **(12) V.** | **Nominal Voltage** | **2.** |
| **200)Ah.)** | **Nominal Capacity** | **3.** |
| **not less than 5years at 20ºC.** | **Design floating Life** | **4** |
| **-10to +55** | **Operating temperature** | **5.** |
| **Above 59 kg** | **Weight** | **6.** |
| **2025** | **Production Year** | **7.** |
| **24 months** | **warranty** | **8.** |

**Quantities:**

**Gel Batteries ( 12 V/ 100 Ah ) Technical Specifications and**

**Quantities:**

|  |  |  |
| --- | --- | --- |
| **Value** | **Parameter** | **No.** |
| **- Gel Type Battery, Deep Cycle**  **- Solar Energy Applications**  **- Completely Maintenance Free.**  **- Sealed construction.** | **Type & Application** | **1.** |
| **(12) V.** | **Nominal Voltage** | **2.** |
| **100)Ah.)** | **Nominal Capacity** | **3.** |
| **not less than 5years at 20ºC.** | **Design floating Life** | **4.** |
| **-10to +55** | **Operating temperature** | **5.** |
| **Above 29 kg** | **Weight** | **6.** |
| **2025** | **Production Year** | **7.** |
| **24 months** | **warranty** | **8.** |